Press Release
New products for Koenig & Bauer commercial presses

New UV coating unit for Koenig & Bauer C16 successfully commissioned

•	New UV coating unit for C16
•	New-level product finishing
•	Intelligent copy control in quarterfold
•	New ribbon lead

Würzburg, 19.06.2018
On the one hand there are short jobs, a raft of different orders and high quality products, and other the other hand the focus is on high-volume print runs – customer demands placed on commercial printers are becoming ever more versatile and challenging. Koenig & Bauer has been successfully tackling both of these developments for years. Stefan Segger, sales director Digital & Web Solutions: “We are in constant communication with our customers. On the one hand we develop new products with our partners, and on the other hand we are proactively represented on the market with new innovations.”
New UV coater for C16 
The new UV coater from Koenig & Bauer offers production speeds of up to 60,000rph, high automation, simple and self-explanatory operation, the stability of a printing unit, automatic cleaning at the push of a button and anilox roller change within a few minutes. Whether for the full-solid finishing of covers or as spot coating for the partial finishing of printed images, the coating unit is already being used very successfully by customers. A compact UV dryer is integrated into the superstructure after the coating unit to enable the widest possible range of paper substrates to be processed. The UV coater processes substrates with a grammage of between 60g/m² - 250g/m² (38 – 160lbs). Between 2 and 5g/m² of coating is applied depending on the anilox roller.
Intelligent copy control in quarterfold
Intelligent, patented copy control in the quarterfold makes for a trouble-free folding sequence. Production conditions are therefore always consistent irrespective of operator skill. Copies are slowed effectively and with a minimum of abrasion, and aligned in the direction of fold during deceleration. The automatic copy control system is self-adjusting and exceptionally reliable regardless of production speed and copy thickness. As a result folding is consistently accurate, even during changes in press speed. Stefan Segger, sales director KBA-Digital & Web Solutions: “We continue to be very successful in the market and expect investments to be made this year. Our presses are known for their quality. With our know-how we have worked on many new developments for our commercial presses.”
Superstructure concept with new ribbon lead
The microporous patented turner bars are one of the many proven features that are unique to Koenig & Bauer. They no longer need to be set for different ribbon widths, and operate reliably with a minimal air cushion and superior ribbon guides. A modular design and dedicated drives throughout allow the superstructure to be customized for specific production scenarios. The short and stable web lead allows a more even web tension.

Photo 1:
New superstructure design with cutting-edge ribbon lead
Photo 2:
New UV coating unit for Koenig & Bauer C16

Press contact
KBA-Digital & Web Solutions AG & Co. KG
Henning Düber
T +49 931 909-4039
M henning.dueber@koenig-bauer.com

About Koenig & Bauer
Koenig & Bauer is the world’s second-largest printing press manufacturer with the broadest product range in the industry. For 200 years, the company has been supporting printers with innovative technology, tailor-made processes and a wide array of services. The portfolio ranges from banknotes, via board, film, metal and glass packaging, through to book, display, coding, magazine, advertising and newspaper printing. Sheetfed and webfed offset and flexo printing, waterless offset, intaglio, simultaneous perfecting and screen printing or digital inkjet – Koenig & Bauer is at home in virtually all printing processes and is the market leader in many of them. In the financial year 2017, the approximately 5,600 highly qualified employees worldwide generated annual sales of more than EUR 1.2 billion.

Further information can be found at www.koenig-bauer.com